Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package josx.platform.rcx

Access to RCX sensors, motors, etc.

See:
Description

Interface Summary
ButtonListener | Abstraction for receiver of button events.
LCDConstants | LCD constants.
ListenerCaller | Interface for calling calling lejos listeners.
Opcode | Opcode constants.
Segment | LCD segment constants.
SensorConstants | Constants for Sensor methods.
SensorListener | Listener of sensor events.
SerialListener | Listener of incomming serial data.

Class Summary
Battery | Provides access to Battery.
Button | Abstraction for an RCX button.
LCD | LCD routines.
Memory | Provides access to memory.
Message | Message API for infra-red (IR) communication that is compatible with the SendMessage command of the LEGO firmware.
MinLCD | Only the most basic APIs from LCD.
MinSound | Only the most basic APIs from Sound.
MinuteTimer | Provides access to Battery.
Motor | Abstraction for a motor.
PersistentMemoryArea | A memory area for persistent storage.
Poll | Provides blocking access to events from the RCX.
ProximitySensor | A 'sensor' to detect object proximity.
ROM | Provides access to ROM routines.
Sensor | Abstraction for a sensor (considerably changed since alpha5).
Serial | Low-level API for infra-red (IR) communication between an RCX and the IR tower or between two RCXs.
Servo | Implmentation of a servo using a Motor and a Rotation Sensor.
Sound | RCX sound routines.
TextLCD | Display text on the LCD screen.

## Package josx.platform.rcx Description

Access to RCX sensors, motors, etc. (Similar to undocumented tinyvm.rcx package).

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES