Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## josx.platform.rcx
Interface SerialListener

All Known Implementing Classes:
  RemoteControlSensor

    public interface SerialListener

Listener of incomming serial data.

See Also:
  `Serial.addSerialListener(josx.platform.rcx.SerialListener)`

Method Summary
`void` | `packetAvailable(byte[] packet, int length)` Called when a packet is received through the IR.

Method Detail

### packetAvailable

    void packetAvailable(byte[] packet,
                         int length)

  Called when a packet is received through the IR.

  Parameters:
    `packet` - The packet data received.
    `length` - The length of the packet.

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD