Our updated Terms of Use will become effective on May 25, 2012. Find out more.

# STL (file format)

From Wikipedia, the free encyclopedia

STL
Filename extension | `.stl`
Developed by | 3D Systems
Type of format | Stereolithography

STL (STereoLithography) is a file format native to the stereolithography CAD software created by 3D Systems. STL is also called as Standard Tessellation Language[1] This file format is supported by many other software packages; it is widely used for rapid prototyping and computer-aided manufacturing. STL files describe only the surface geometry of a three dimensional object without any representation of color, texture or other common CAD model attributes. The STL format specifies both ASCII and binary representations. Binary files are more common, since they are more compact [2].

An STL file describes a raw unstructured triangulated surface by the unit normal and vertices (ordered by the right-hand rule) of the triangles using a three-dimensional Cartesian coordinate system.

## [edit] ASCII STL

An ASCII STL file begins with the line:

    solid name

where name is an optional string (though if name is omitted there must still be a space after solid). The file continues with any number of triangles, each represented as follows:

    facet normal ni nj nk
    outer loop
    vertex v1x v1y v1z
    vertex v2x v2y v2z
    vertex v3x v3y v3z
    endloop
    endfacet

where each n or v is a floating point number in sign-mantissa 'e'-sign-exponent format, e.g., "-2.648000e-002". The file concludes with:

    endsolid name

The structure of the format suggests that other possibilities exist (e.g., facets with more than one 'loop', or loops with more than three vertices) but in practice, all facets are simple triangles.

White space (spaces, tabs, newlines) may be used anywhere in the file except within numbers or words. The spaces between 'facet' and 'normal' and between 'outer' and 'loop' are required.[2]

## [edit] Binary STL

Because ASCII STL files can become very large, a binary version of STL exists. A binary STL file has an 80 character header (which is generally ignored – but which should never begin with 'solid' because that will lead most software to assume that this is an ASCII STL file). Following the header is a 4 byte unsigned integer indicating the number of triangular facets in the file. Following that is data describing each triangle in turn. The file simply ends after the last triangle.

Each triangle is described by twelve 32-bit-floating point numbers: three for the normal and then three for the X/Y/Z coordinate of each vertex – just as with the ASCII version of STL. After the twelve floats there is a two byte unsigned 'short' integer that is the 'attribute byte count' – in the standard format, this should be zero because most software does not understand anything else.[2]

Floating point numbers are represented as IEEE floating point numbers and the endianness is assumed to be little endian although this is not stated in documentation.

    UINT8[80] – Header
    UINT32 – Number of triangles

    foreach triangle
    REAL32[3] – Normal vector
    REAL32[3] – Vertex 1
    REAL32[3] – Vertex 2
    REAL32[3] – Vertex 3
    UINT16 – Attribute byte count
    end

## [edit] Colour in binary STL

There are at least two variations on the binary STL format for adding colour information:

- The VisCAM and SolidView software packages use the two 'attribute byte count' bytes at the end of every triangle to store a 15 bit RGB colour:
  - bit 0 to 4 are the intensity level for blue (0 to 31)
  - bits 5 to 9 are the intensity level for green (0 to 31)
  - bits 10 to 14 are the intensity level for red (0 to 31)
    - bit 15 is 1 if the colour is valid
    - bit 15 is 0 if the colour is not valid (as with normal STL files)

- The Materialise Magics software does things a little differently. It uses the 80 byte header at the top of the file to represent the overall colour of the entire part. If colour is used, then somewhere in the header should be the ASCII string "COLOR=" followed by four bytes representing red, green, blue and alpha channel (transparency) in the range 0–255. This is the colour of the entire object unless overridden at each facet. Magics also recognizes a material description; a more detailed surface characteristic. Just after "COLOR=RGBA" specification should be another ASCII string ",MATERIAL=" followed by three colours (3 × 4 bytes): first is a colour of diffuse reflection, second is a colour of specular highlight, and third is an ambient light. Material settings are preferred over colour. The per-facet colour is represented in the two 'attribute byte count' bytes as follows:
  - bit 0 to 4 are the intensity level for red (0 to 31)
  - bits 5 to 9 are the intensity level for green (0 to 31)
  - bits 10 to 14 are the intensity level for blue (0 to 31)
    - bit 15 is 0 if this facet has its own unique colour
    - bit 15 is 1 if the per-object colour is to be used

The red/green/blue ordering within those two bytes is reversed in these two approaches – so whilst these formats could easily have been compatible the reversal of the order of the colours means that they are not – and worse still, a generic STL file reader cannot automatically distinguish between them. There is also no way to have facets be selectively transparent because there is no per-facet alpha value – although in the context of current rapid prototyping machinery, this is not important.

## [edit] The facet normal

In both ASCII and binary versions of STL, the facet normal should be a unit vector pointing outwards from the solid object. In most software this may be set to (0,0,0) and the software will automatically calculate a normal based on the order of the triangle vertices using the 'right-hand rule'. Some STL loaders (e.g. the STL plugin for Art of Illusion) check that the normal in the file agrees with the normal they calculate using the right-hand rule and warn you when it does not. Other software may ignore the facet normal entirely and use only the right-hand rule. Although it is rare to specify a normal that cannot be calculated using the right-hand rule, in order to be entirely portable, a file should both provide the facet normal and order the vertices appropriately. A notable exception is SolidWorks which uses the normal for shading effects.

## [edit] History of use

Stereolithography machines are basically 3D printers that can build any volume shape as a series of slices. Ultimately these machines require a series of closed 2D contours that are filled in with solidified material as the layers are fused together.

The natural file format for such a machine would be a series of closed polygons corresponding to different Z-values. However, since it's possible to vary the layer thicknesses for a faster though less precise build, it seemed easier to define the model to be built as a closed polyhedron that could be sliced at the necessary horizontal levels.

The STL file format appears capable of defining a polyhedron with any polygonal facet, but in practice it's only ever used for triangles, which means that much of the syntax of the ASCII protocol is superfluous.

STL files are supposed to be closed and connected like a combinatorial surface, where every edge is part of exactly two triangles, and not self-intersecting. Since the syntax does not enforce this property, it can be ignored for applications where the closedness doesn't matter.

The closedness only matters insofar as the software which slices the triangles requires it to ensure that the resulting 2D polygons are closed. Sometimes such software can be written to clean up small discrepancies by moving endpoints of edges that are close together so that they coincide. The results are not predictable, but it is often sufficient to get the job done.

## [edit] Use in other fields

Many computer-aided design systems are able to output the STL file format among their other formats because it's quick and easy to implement, if you ignore the connection criteria of the triangles. Many computer-aided manufacturing systems require triangulated models as the basis of their calculation.

Since an STL file output, of a sorts, is almost always available from the CAD system, it's often used as a quick method for importing the necessary triangulated geometry into the CAM system.

It can also be used for interchanging data between CAD/CAM systems and computational environments such as Mathematica.

Once it works, there is very little motivation to change, even though it is far from the most memory and computationally efficient method for transferring this data. Many integrated CAD and CAM systems transfer their geometric data using this accidental file format, because it's impossible to go wrong.

There are many other file formats capable of encoding triangles available, such as VRML, DXF, but they have the disadvantage that it's possible to put things other than triangles into it, and thus produce something ambiguous or unusable.

## [edit] See also

- Additive Manufacturing File Format, an ASTM standard that has native support for color, multiple materials, and constellations
- PLY (file format), an alternative file format offering more flexibility than most stereolithography applications.
- Wavefront .obj file, a 3D geometry definition file format with .obj file extension
- MeshLab, a free and open source cross-platform application for visualizing, processing and converting three-dimensional meshes to or from the STL file format.
- Mathematica, a technical computing system that can work with PLY files.

## [edit] References

1. ^ http://www.rapidtoday.com/stl-file-format.html
2. ^ a b c Burns, Marshall (1993). Automated Fabrication. Prentice Hall. ISBN 978-0-13-119462-5.

- StereoLithography Interface Specification, 3D Systems, Inc., July 1988
- StereoLithography Interface Specification, 3D Systems, Inc., October 1989
- SLC File Specification, 3D Systems, Inc., 1994
- Chua, C. K; Leong, K. F.; Lim, C. S. (2003), Rapid Prototyping: Principles and Applications, World Scientific Publishing Co, ISBN 981-238-117-1 Chapter 6, Rapid Prototyping Formats. Page 237, "The STL (STeroLithography) file, as the de facto standard, has been used in many, if not all, rapid prototyping systems." Section 6.2 STL File Problems. Section 6.4 STL File Repair.

## [edit] External links

- The StL Format: Standard Data Format for Fabbers
- Instructions for exporting STL files from various CAD packages (courtesy of ProtoCAM)

Retrieved from "http://en.wikipedia.org/w/index.php?title=STL_(file_format)&oldid=492009558"
View page ratings
Rate this page
Rate this page
Page ratings
What's this?
Current average ratings.
Trustworthy
Objective
Complete
Well-written
I am highly knowledgeable about this topic (optional)
I have a relevant college/university degree
It is part of my profession
It is a deep personal passion
The source of my knowledge is not listed here
I would like to help improve Wikipedia, send me an e-mail (optional)
We will send you a confirmation e-mail. We will not share your e-mail address with outside parties as per our feedback privacy statement.
Saved successfully
Your ratings have not been submitted yet
Your ratings have expired
Please reevaluate this page and submit new ratings.
An error has occurred. Please try again later.
Thanks! Your ratings have been saved.
Please take a moment to complete a short survey.
Thanks! Your ratings have been saved.
Do you want to create an account?
An account will help you track your edits, get involved in discussions, and be a part of the community.
or
Thanks! Your ratings have been saved.
Did you know that you can edit this page?
Categories:

- 3D printing
- CAD file formats
- Graphics file formats
- Computer file formats
- 3D computer graphics

##### Personal tools

- Log in / create account