Subject: cilco pathing - withdrawl and hplc transport pathing
cilco needs to be pathed the following way on a withdrawl day or month
the pathing that was done for december 1999 and january 2000 worked .
source
path
destination
012 - 27049 - 05 - 001 / stg / f 012 - 27049 - 05 - 001
firm storage external
bammel - meter 56 l
storage
account
meter 56 must be attached to this pool
external bammel - meter 56 012 - 27049 - 02 - 001
transport
012 - 27049 - 02 - 001 / transport / i / 1 / e
meter 56 must be
attached
transport imbalance
the hplc transport in or out of storage should be pathed as follows
injection
source
path
destination
012 - 41500 - 02 - 015 / transport / i / 1 / e
012 - 41500 - 02 - 015
external bammel - meter 57
transport
imbalance
meter 57 must be attached to this pool
withdrawl
external bammel - meter 57
012 - 41500 - 02 - 015
012 - 41500 - 02 - 015 / transport / i / 1 / e
meter 57 must be attached to this
pool
transport imbalance